[root@RHIS-CR-0613-03 cssd]# ethtool eth3
Settings for eth3:
        Supported ports: [ FIBRE ]
        Supported link modes:   1000baseT/Full
                               10000baseT/Full
        Supports auto-negotiation: Yes
        Advertised link modes:  1000baseT/Full
                                10000baseT/Full
        Advertised auto-negotiation: Yes
        Speed: 10000Mb/s
        Duplex: Full
        Port: FIBRE
        PHYAD: 1
        Transceiver: internal
        Auto-negotiation: on
        Supports Wake-on: g
        Wake-on: g
        Current message level: 0x00000000 (0)
        Link detected: yes
